GB |
Z6F 6 65A12C | HEADLIGHT HARNESS

INJECTION ZPJ ZPJ4 LEFT HAND DRIVE EXCEPT AIR CONDITIONING

FRONT HARNESS
01 | 6511 FC | 01 | MAIN HARNESS MARK 9612839380 - LEVEL 2 SPEED CONTROL ANTI-START CODE UP TO 12/1991
| 6511 KK | 01 | MARK 9615438080 - LEVEL 2 SPEED CONTROL ANTI-START CODE SINCE 12/1991 UP TO 06/1992
| 6511 KJ | 01 | MARK 9615763480 - LEVEL 2 SPEED CONTROL ANTI-START CODE SINCE 06/1992 UP TO 03/1993
| 6502 RK | 01 | MARK 9617271380 9619772380 - LEVEL 2 SPEED CONTROL ANTI-START CODE WITHOUT AIR CONDITIONING SINCE 03/1993
02 | 6511 GJ | 01 | MARK 9612839880 - LEVEL 3 SPEED CONTROL ANTI-START CODE UP TO 06/1992 AFTER 6/92 USE 6511 KQ
03 | 6502 Q6 | 01 | MARK 9612839680 9612840280 - LEVEL 4 SPEED CONTROL ANTI-START CODE UP TO 06/1992

6511 KQ

01

MARK
9615438180
9615438280
9615764280
- LEVEL 3 SPEED CONTROL ANTI-START CODE SINCE 06/1992
- LEVEL 4 SPEED CONTROL ANTI-START CODE SINCE 06/1992

20 | 6500 34 | 01 | CONNECTR BRACKT
21 | 6500 81 | 01 | SOCKET BRACKET
30 | 6500 A0 | 01 | CONNECTR BRACKT - PETROL UP TO 04/1993
| 6555 GN | 01 | - PETROL SINCE 04/1993
31 | 6555 GK | 01 | SIERA
40 | 6542 94 | 01 | EARTH CONTACT A=5
70 | 6992 A7 | 01 | CLIP DIAM 13
71 | 6992 C2 | 01 | DIAM 12
72 | 6992 A8 | 01 | 1,5-3--6,5
73 | 6995 05 | 01 |
74 | 6980 28 | 01 | STRAP L=275 LARG=5
75 | 6980 47 | 01 | LONG 171 LARG 9
76 | 6980 33 | 01 | LONG=150 LARG=7
77 | 6924 88 | 01 | SCREW WITH BASE 6X100-22