GB |
Z6F 1 13E10A | RADIATOR WATER HOSE WATER TANK

PETROL XU10

01 | 1336 69 | 01 | OUTLET TANK - MECHANICAL FUEL PUMP ASSEMBLY UP TO 12/1990
| 1336 70 | 01 | - INJECTION UP TO MOD 1991 - CARBURETTOR XU102C ELECTRIC FUEL PUMP ASSEMBLY UP TO 12/1990
| 1336 99 | 01 | - XU102C ELECTRIC FUEL PUMP ASSEMBLY SINCE 12/1990 - XU102C MECHANICAL FUEL PUMP ASSEMBLY SINCE 12/1990 UP TO 05/1992
| 1336 E3 | 01 | - XU102C MECHANICAL FUEL PUMP ASSEMBLY SINCE 05/1992
| 1336 C6 | 01 | - XU10J2 SINCE MOD 1991 - XU10M SINCE MOD 1991 - TURBO INJECTION XU10J2TE
02 | 1306 29 | 02 | DRAIN SCREW - INJECTION UP TO MOD 1991 - CARBURETTOR XU102C UP TO 12/1990 - INJECTION SINCE MOD 1991 - CARBURETTOR XU102C SINCE 12/1990
03 | 1336 33 | 01 | SOCKET SCREW 7X100-55
04 | 1336 G0 | 01 | WATER OUTLET - INJECTION UP TO MOD 1991 - CARBURETTOR XU102C UP TO 12/1990
| 1336 A1 | 01 | - INJECTION SINCE MOD 1991 - CARBURETTOR XU102C SINCE 12/1990

05

1338 11

01

THERMOSTAT
89 DEG
DAUPHIN THOMSON
VERNET V1931
- BVM
- BVA UP TO 01/1993

| 1338 37 | 01 | 82 DEG (83 DEG) DAUPHIN THOMSON VERNET VERNET V1725C - BVA EXCEPT (GE) SINCE 01/1993
| 1338 83 | 01 | 82 DEG (83 DEG) DAUPHIN THOMSON VERNET VERNET V1725C - BVA (GE) SINCE 01/1993
06 | 1339 10 | 02 | THERMOST GASKET - INJECTION UP TO MOD 1991 - CARBURETTOR XU102C UP TO 12/1990
| 1340 30 | 01 | - INJECTION SINCE MOD 1991 - CARBURETTOR XU102C SINCE 12/1990
07 | 1339 64 | 01 | HOUSING SEAL
08 | 8249 18 | 02 | SEAL WASHER DIAM 6 - INJECTION UP TO MOD 1991 - CARBURETTOR XU102C UP TO 12/1990 - INJECTION SINCE MOD 1991 - CARBURETTOR XU102C SINCE 12/1990
09 | 1338 09 | 01 | TEMPERATURE 110 DEG JAEGER BE BLUE - AIR CONDITIONING EXCEPT TURBO INJECTION XU10J2TE
| 1338 34 | 01 | BE BLUE - TURBO INJECTION XU10J2TE
| 1338 15 | 01 | TEMPERAT. PROBE 105 DEGRES JAEGER BA WHITE - CARBURETTOR EXCEPT AIR CONDITIONING
| 0242 76 | 01 | 14X1,25-48ø JAEGER NR BLACK - INJECTION EXCEPT AIR CONDITIONING EXCEPT TURBO INJECTION XU10J2TE
10 | 0242 68 | 01 | 14X1,25-118 DEG JAEGER ELTH BE BLUE - EXCEPT AIR CONDITIONING EXCEPT TURBO INJECTION XU10J2TE
| 1338 55 | 01 | SENSOR 14X125 ELECTRICFIL MR MAROON - AIR CONDITIONING
| 1338 56 | 01 | TEMPERATURE MR MAROON - TURBO INJECTION XU10J2TE
11 | 1920 C4 | 01 | TEMPERAT. PROBE - INJECTION EXCEPT TURBO INJECTION XU10J2TE
12 | 0242 74 | 01 | WATER TEMP CASE 118ø BITRON VIDEO - XU102C AIR CONDITIONING - TURBO INJECTION XU10J2TE BVM
| 0242 73 | 01 | 118ø BITRON VIDEO - XU10J2 AIR CONDITIONING
| 0242 80 | 01 | 118ø BITRON VIDEO - TURBO INJECTION XU10J2TE BVA
13 | 5404 02 | 01 | VALVE PLUG - INJECTION SINCE MOD 1991 - CARBURETTOR XU102C SINCE 12/1990
14 | 1336 K8 | 01 | WATER OUTLET
70 | 6968 40 | 01 | PIN 10X13
71 | 6922 22 | 02 | SELF-TAP SCREWS 8X125-20 - EXCEPT TURBO INJECTION XU10J2TE - TURBO INJECTION XU10J2TE
| 1336 F0 | 01 | SCREW COLUMN M8X125-M6X100 - TURBO INJECTION XU10J2TE
72 | 6922 85 | 01 | SELF-TAP SCREWS 7X100-40
73 | 6923 20 | 01 | 7X100-55
74 | 6923 19 | 01 | 7X100-75