GB |
Z7F 4 40H65A | HP/BP PIPING

INJECTION XU10J4R POWER ASSISTED STEERING LEFT HAND DRIVE
UP TO O 7144

01 | 4020 GJ | 01 | LOW PRESS PIPE - WITHOUT AIR CONDITIONING
| 4020 0V | 01 | - AIR CONDITIONING
02 | 4020 9T | 01 | HIGH PRES FLEXB - WITHOUT AIR CONDITIONING
| 4020 1V | 01 | - AIR CONDITIONING
03 | 4018 68 | 02 | LINE BRACKET - WITHOUT AIR CONDITIONING - AIR CONDITIONING
04 | 4010 31 | 01 | SCREW COLUMN 8X125-24/7X100-14
05 | 4020 X3 | 02 | TUBE RING - WITHOUT AIR CONDITIONING - AIR CONDITIONING
06 | 4018 E4 | 01 | LINE BRACKET
07 | 4018 E5 | 02 |
09 | 4020 0S | 01 | LOW PRESS PIPE
| RP 4020 GW | 01 |
10 | 4020 CX | 01 |
70 | 6992 F1 | 01 | CLIP DIAM 15-25 - WITHOUT AIR CONDITIONING
71 | 6981 83 | 02 | METALLIC CLAMP DIAM 16-27 LARG 9
72 | 6924 93 | 01 | CAPSCREW 8X125-20
73 | 6932 38 | 02 | HEXAGONAL NUT 8X125-6,5
74 | 6936 71 | 02 | WASHER-NUT 8X125-9-22
75 | 6934 04 | 02 | HEXAGONAL NUT 6X100-3
76 | 6981 82 | 01 | METALLIC CLAMP DIAM 11-19 LARG 9