GB |
Z7F 6 60D16B | ENGINE WIRING

INJECTION XU10J4R BVA

01 | 6544 9W | 01 | ENGINE HARNESS MARK 9621427580 - RIGHT HAND DRIVE STANDARD IGNITION UP TO S 91029025
| 6544 1X | 01 | MARK 9621427680 - LEFT HAND DRIVE UP TO S 91029025 - RIGHT HAND DRIVE CODED IGNITION UP TO S 91029025
| 6544 WR | 01 | MARK 9626484080 - RIGHT HAND DRIVE STANDARD IGNITION SINCE S 91029026 UP TO O 7069
| 6544 HP | 01 | MARK 9624333980 - LEFT HAND DRIVE SINCE S 91029026 UP TO O 7069 - RIGHT HAND DRIVE CODED IGNITION SINCE S 91029026 UP TO O 7069
| 6549 59 | 01 | MARK 9626483280 - RIGHT HAND DRIVE STANDARD IGNITION EXCEPT DEPOL 15-04 SINCE O 7070 UP TO O 7147
| 6549 60 | 01 | MARK 9626416380 - CODED IGNITION EXCEPT DEPOL 15-04 SINCE O 7070 UP TO O 7147

6549 CL

01

MARK
9626416580
9627217480
9628977880
- LEFT HAND DRIVE STANDARD IGNITION SINCE O 7070 UP TO O 7147
- RIGHT HAND DRIVE STANDARD IGNITION DEPOL 15-04 SINCE O 7070 UP TO O 7147
- CODED IGNITION DEPOL 15-04 SINCE O 7070 UP TO O 7147
SINCE O 7148
UP TO O 7874

05 | 6544 AS | 01 | HARNESS-REHEAT MARK 9622778680 UP TO O 7875
11 | 6555 TJ | 01 | BRACKET EP 1,3
12 | 6555 TK | 01 | EP 2,5
13 | 6555 TL | 01 |
14 | 6500 81 | 01 | SOCKET BRACKET
15 | 6555 GK | 01 | CONNECTR BRACKT SIERA
17 | 6500 23 | 01 | PLASTIC NUT 23 VOIES
18 | 6500 68 | 01 | 14 VOIES
20 | 6500 33 | 01 | HARNESS BRACKET
68 | 6992 A6 | 01 | CLIP DIAM 6-12
69 | 6555 LY | 01 | HARNESS CLIP DIAM 6 --6,2-12,2
70 | 6995 26 | 01 | CLIP DIAM 12
71 | 6995 08 | 01 | L=6,2X12,2
72 | 6992 A7 | 01 | DIAM 13
73 | 6992 39 | 01 | SWIVEL CLIP DIAM 18-20
| RP 6994 68 + 6994 69 | 01 01 |
75 | 6547 08 | 01 | STRAP L=200 LARG=5
| RP 6981 G9 | 01 |
76 | 6980 30 | 01 | LONG 100
78 | 6936 91 | 01 | NUT WITH BASE 6 X 100 - 6 - 10
| RP 6936 A0 | 01 |
81 | 6936 35 | 04 | 8X125