GB |
Z6F 6 65A11A | PRICIPAL HARNESS

(I) ITALY

01

6502 L9

01

MAIN HARNESS
MARK
9610828380
9610828480
9610828680
9611117380
9611117480
- INJECTION XU10J2 AIR CONDITIONING EXCEPT VARIABLE POWER STEERING EXCEPT ANTI-START CODE SINCE MOD 1990 UP TO 04/1991

6511 FD

01

MARK
9612838280
9615151580
- INJECTION XU10M LEVEL 1 AIR CONDITIONING SINCE 04/1991 UP TO 06/1992
- INJECTION XU10J2 LEVEL 2 AIR CONDITIONING SINCE 04/1991 UP TO 06/1992
- DIESEL D11ATE LEVEL 2 AIR CONDITIONING SINCE 04/1991 UP TO 06/1992

| 6511 KH | 01 | MARK 9615763180 - INJECTION XU10J2 LEVEL 2 AIR CONDITIONING SINCE 06/1992 UP TO 03/1993 - DIESEL D11ATE LEVEL 2 AIR CONDITIONING SINCE 06/1992 UP TO 03/1993
| 6502 RJ | 01 | MARK 9617271280 9619772280 - INJECTION XU10J2 LEVEL 2 AIR CONDITIONING THEFT PROTECTION ALARM SINCE 03/1993 - DIESEL D11ATE LEVEL 2 AIR CONDITIONING THEFT PROTECTION ALARM SINCE 03/1993
02 | 6502 M0 | 01 | MARK 9610828580 - INJECTION XU10J2 BVA EXCEPT AIR CONDITIONING EXCEPT VARIABLE POWER STEERING EXCEPT ANTI-START CODE SINCE MOD 1990 UP TO 04/1991
| 6502 P9 | 01 | MARK 9612838880 9615157480 - INJECTION XU10J2 LEVEL 3 EXCEPT AIR CONDITIONING SINCE 04/1991 UP TO 06/1992
| 6511 KN | 01 | MARK 9615763980 - INJECTION XU10J2 LEVEL 3 EXCEPT AIR CONDITIONING SINCE 06/1992
03 | 6502 P8 | 01 | MARK 9612838980 9615157580 - INJECTION XU10J2 LEVEL 3 AIR CONDITIONING SINCE 04/1991 UP TO 06/1992
| 6511 KP | 01 | MARK 9615764080 - INJECTION XU10J2 LEVEL 3 AIR CONDITIONING SINCE 06/1992
10 | 6500 81 | 01 | SOCKET BRACKET
11 | 6500 34 | 01 | CONNECTR BRACKT UP TO 01/1991 FOR CONNECTOR
12 | 6500 A0 | 01 | - PETROL SINCE 01/1991 FOR ROUND CONNECTORS
13 | 6542 94 | 01 | EARTH CONTACT A=5 10 POINT
70 | 6992 A7 | 01 | CLIP DIAM 13
71 | 6992 C2 | 01 | DIAM 12
73 | 6992 A8 | 01 | 1,5-3--6,5
74 | 6995 05 | 01 |
80 | 6983 59 | 01 | WIRING SHEATH 22-70-45
| 6555 GF | 01 | RIGHT DRAFTEX - EXCEPT WITH ABS BRAKES
| 6555 GE | 01 | RIGHT DRAFTEX - WITH ABS BRAKES
81 | 6983 60 | 01 | PLUG
82 | 6555 H9 | 01 | COVER RIGHT
| 6555 JA | 01 | RIGHT
83 | 6500 99 NFP | 01 | WIRING SHEATH LEFT
| 6555 GC | 01 | LEFT DRAFTEX
84 | 7938 15 | 01 | PLUG
85 | 6555 H8 | 01 | COVER LEFT
| 6555 JG | 01 | LEFT
86 | 1628 W0 | 01 | SPACER
87 | 6939 97 | 01 | WASHER-NUT 6 X 100 - 7 - 18