GB |
Z7F 1 12C85A | ENGINE MOTOR DRIVEN FAN TUBE

TURBO DIESEL DK5ATE

01 | 1253 29 | 02 | MOTOR DRIVN FAN 310 W ECIA - UP TO 07/1995
| 1253 55 | 02 | 310W GATE - SINCE 07/1995
02 | 1254 67 | 02 | MOTOR DRIV FAN DIAM 300 ECIA - UP TO 07/1995
| 1254 66 | 02 | 6 PALES GATE * SINCE 07/1995
03 | 1338 51 | 01 | GMP ELECTRI BOX BITRON VIDEO - WITHOUT AIR CONDITIONING UP TO 06/1995
| 1338 62 | 01 | WATER TEMP CASE
| RP 1338 96 | 01 | BITRON VIDEO - WITHOUT AIR CONDITIONING SINCE 06/1995
| 1338 45 | 01 | GMP ELECTRI BOX BITRON VIDEO - AIR CONDITIONING UP TO 06/1995
| 1338 59 | 01 | REGULATOR BOX 96ø/118ø
| RP 1338 81 | 01 | BITRON VIDEO GR GREY - AIR CONDITIONING SINCE 06/1995
04 | 6455 Q0 | 03 | ELECTRIC RELAY 25 AMP
| RP 6555 68 | 01 | NR BLACK UP TO 07/1995
| 6547 TX | 03 | 35 AMP FAN MOTOR WITH RESISTANCE
05 | 0163 53 | 01 | PLUG 22X150
06 | 0243 18 | 01 | SEAL 22,4X30-2 A005 WITHOUT ASBESTOS
07 | 1254 62 | 02 | FIXING CLIP SINCE 07/1995
70 | 6905 61 | 02 | CAPSCREW 4X70-10 PAS A GAUCHE
71 | 6957 14 | 02 | SPRING WASHER 4X11,2-0,6
72 | 6922 87 | 06 | SCREW WITH BASE 6X100-22
73 | 6925 33 | 02 | SCREW CBLX RDL 5X80-16