GB |
Z7F 1 11A10A | ENGINE OIL SUMP FILTER PROBE

TURBO INJECTION XU10J2TE BVM WITHOUT AIR CONDITIONING

01 | 1109 N2 | 01 | OIL FILTER LS 867B PURFLUX- -
02 | 0301 C5 | 01 | ENGINE OIL SUMP
03 | 0311 21 | 01 | CYL-BLOCK PLUG 14X125
04 | 0313 27 | 01 | HOUSG PLUG SEAL 14X21-2 A005 WITHOUT ASBESTOS
05 | 1131 70 | 01 | OIL LEVEL PROBE
06 | 0243 01 | 01 | SWITCH GASKET 18,4X23-1,2 A005 WITHOUT ASBESTOS
07 | 1186 08 | 01 | FILTER ELEMENT
08 | 1174 08 | 01 | ENGINE OIL GAUG
09 | 1171 80 | 01 | OIL GAUGE GUIDE SUP
10 | 1171 73 | 01 | INF
11 | 1103 C9 | 01 | DISTRIB CHAMBER EP=47,6 SOLEX MODINE
12 | 1104 24 | 01 | SEAL 66,80X73,66-3,43 MODINE -
| 1104 19 | 01 | 62,3X71,8-4,75 VALEO THERMIQUE -
13 | 1103 C6 | 01 | OIL FILT INSERT LONG 70
14 | 1131 82 | 01 | OIL PRES SWITCH 16X150 JAEGER SOBINT UP TO O 7874
15 | 1168 10 | 01 | LUBRICATN PIPE
16 | 1166 21 | 05 | RING-SEAL
17 | 0609 04 | 04 | PISTON OIL JET
| RP 0609 10 + 0307 13 | 01 01 | UP TO O 7664
| 0609 10 | 04 | SINCE O 7665
18 | 0610 02 | 04 | OIL JET SCREW 6X100-27 UP TO O 7664
| 0307 13 | 04 | SCREW WITH BASE 6X100-18 SINCE O 7665
19 | 1131 80 | 01 | TEMPERATURE 14X125 - 155DEG BE BLUE
70 | 6928 01 | 23 | SCREW WITH BASE 7X100-15