GB |
Z7F 1 13A10A | COOLING RADIATOR

INJECTION XU10J4R

01 | 1300 L9 | 01 | RADIATOR NEW - BVM WITHOUT AIR CONDITIONING EXCEPT (IL)
| 1301 KL | 01 | RADIAT EXCHANGE - BVM (F) FRANCE WITHOUT AIR CONDITIONING 1ST POSSIBILITY "CHAUSSON"
| 1301 NF | 01 | - BVM (F) FRANCE WITHOUT AIR CONDITIONING 2ND POSSIBILITY "RADIA-FRANCE"
| 1301 A1 | 01 | - BVM (EUR) EUROPE WITHOUT AIR CONDITIONING EXCEPT (F) FRANCE
| 1300 N0 | 01 | RADIATOR NEW - BVM (IL) - BVM AIR CONDITIONING
| 1331 E9 | 01 | RADIAT EXCHANGE - BVM (F) FRANCE AIR CONDITIONING 1ST POSSIBILITY "CHAUSSON"
| 1301 ZH | 01 | - BVM (F) FRANCE AIR CONDITIONING 2ND POSSIBILITY "RADIA-FRANCE"
| 1301 A5 | 01 | - BVM (EUR) EUROPE AIR CONDITIONING EXCEPT (F) FRANCE
| 1301 X5 | 01 | RADIATOR NEW - BVA
| 1301 LZ | 01 | RADIAT EXCHANGE - BVA (F) FRANCE 1ST POSSIBILITY "CHAUSSON"
| 1301 PS | 01 | - BVA (F) FRANCE 2ND POSSIBILITY "RADIA-FRANCE"
| 1301 X7 | 01 | - BVA (EUR) EUROPE EXCEPT (F) FRANCE
02 | 1306 84 | 01 | FILLER PLUG 1,4 BAR BAILLY COMTE UP TO 07/1995
| 1306 99 | 01 | 1,4 BAR
| RP 1306 C7 | 01 | SINCE 07/1995
03 | 1312 82 | 02 | RETAING SPRING
04 | 1313 06 | 02 | RUBBER BUFFER DIAM EXT 26 EP 19
05 | 1306 68 | 01 | LEVEL DETECTOR - BVM WITHOUT AIR CONDITIONING EXCEPT (IL)
06 | 1306 77 | 01 | DRAIN PLUG DIAM 14 VALEO (THERMIQ) -