GB |
Z6F 0 02A30A | CYLINDER-HEAD GUIDE AND VALVE SEAT

DIESEL XU

A) SEE SERVICE INFO Nø 164 DATED 11/95
01 | 0200 A8 | 01 | CYLINDER-HEAD
| RP 0200 T1 | 01 |
| 0200 Q7 | 01 | - XUD11A WITH VALVES AND CAMSHAFT
| 0200 Q8 | 01 | - D11ATE WITH VALVES AND CAMSHAFT
| 0200 R2 | 01 | CARCASE WITH VALVES AND CAMSHAFT
02 | 0204 67 | 01 | CYL-HEAD SCREW - XUD11A - D11ATE UP TO 02/1992
| 0204 68 | 01 | - D11ATE SINCE 02/1992
03 | 0205 30 | 10 | PLAIN WASHER
04 | 0209 T6 | 01 | CYL HEAD GASKET A005 WITHOUT ASBESTOS - D11ATE HOLES 1 AND 2 PIERCED (FITTED DEPTH 1,35) - SEE A
05 | 0209 R5 | 01 | CLASSE 2 A005 WITHOUT ASBESTOS - D11ATE
06 | 0209 R6 | 01 | CLASSE 3 A005 WITHOUT ASBESTOS - D11ATE
07 | 0209 R7 | 01 | CLASSE 4 A005 WITHOUT ASBESTOS - D11ATE
08 | 0209 H1 | 01 | EP 1,5 REINZ A005 WITHOUT ASBESTOS - XUD11A
09 | 0209 99 | 01 | EP 1,60 REINZ A005 WITHOUT ASBESTOS - XUD11A
10 | 0209 A0 | 01 | EP 1,70 REINZ A005 WITHOUT ASBESTOS - XUD11A
11 | 0209 H3 | 01 | EP 1,80 A005 WITHOUT ASBESTOS - XUD11A