GB |
Z7F 2 23A60A | FIRST LINE MANUAL GEAR BOX

BVM MG5T

A) WITHOUT GROOVE MARK BETWEEN 3RD AND
4TH
B) 2 GROOVE MARKS SITUATED AT 30MM AND
40MM FROM THE EXT FACE OF THE
4TH GEAR
C) ORDER IF REQUIRED THE SYNCHRONIZER
REF 2388 13

01 | 2311 F8 | 01 | PRIMARY SHAFT 12X23X34X43 - INJECTION ZPJ SEE A) AND SEE C) - INJECTION ZPJ4
| 2311 G0 | 01 | 12X22X34X43 - TURBO DIESEL DK5ATE
02 | 2304 37 | 01 | SHAFT FIX NUT 24X150
| RP 2304 47 | 01 |
03 | 2304 38 | 01 | WASHER DIAM 24,5X49
04 | 2370 57 | 01 | SLIDING GEAR 29 DTS (12X29)
05 | 2372 41 LE-9702 | 01 | SHAFT BEARING 27X52-17,35
06 | 2373 11 LE-9803 | 01 | 34X62-17
07 | 2306 24 LE-9702 | 01 | ADJUST SHIM SET
08 | 2375 40 | 01 | RING
09 | 2382 39 | 01 | RETURN SHAFT
11 | 2385 22 | 01 |
12 | 2538 07 | 02 | LOCKING BALL DIAM 8
13 | 2385 23 | 01 | GEAR SHAF SCREW 8X125-55
14 | 2385 24 | 01 | SHAFT SEAL DIAM 9,2X15-1
15 | 2372 52 | 01 | PRIMARY KIT
70 | 6969 39 | 01 | PIN 5X35 UP TO 12/1994
| 6969 38 | 01 | 5X25 SINCE 12/1994