GB |
Z7F 0 01A10A | ENGINE

INJECTION XU

A) IF REQUIRED RECOVER OR CHANGE THE
OIL SUMP
B) IF REQUIRED RECOVER OR CHANGE THE
BAFFLE ANTI SURGE OIL PUMP + THE
OIL GAUGE
C) IF REQUIRED CHANGE ENGINE SUPPORT
LOWER RH
D) FOR BVA : CHANGE OR RECOVER THE
ENGINE SUPPORT INTERMEDIATE RH

01 | 0135 J5 | 01 | NEW ENGINE A005 WITHOUT ASBESTOS MARK R6A - INJECTION XU10J2
| 0135 Y7 | 01 | MARK RGX RGY - TURBO INJECTION XU10J2TE UP TO 06/1995
| 0139 P4 | 01 | EXCHANGE ENGINE MARK RGX RGY - TURBO INJECTION XU10J2TE UP TO 06/1995
| 0135 6F | 01 | NEW ENGINE
| RP 0135 0V | 01 | MARK RGX - TURBO INJECTION XU10J2TE SINCE 06/1995 UP TO O 8133
| 0139 W0 | 01 | EXCHANGE ENGINE - TURBO INJECTION XU10J2TE SINCE 06/1995 UP TO O 8133
| 0135 0L | 01 | NEW ENGINE MARK RFV - INJECTION XU10J4R BVM EXCEPT DEPOL 15-04 UP TO O 7146 - INJECTION XU10J4R BVA EXCEPT DEPOL 15-04 UP TO O 7664
| 0139 Q7 | 01 | EXCHANGE ENGINE MARK RFV - INJECTION XU10J4R EXCEPT DEPOL 15-04 UP TO 11/1995
| 0139 Y3 | 01 | MARK RFV - INJECTION XU10J4R BVM EXCEPT DEPOL 15-04 SINCE 11/1995 UP TO O 7146 - INJECTION XU10J4R BVA EXCEPT DEPOL 15-04 UP TO O 7664
| 0135 6H | 01 | NEW ENGINE MARK R6E - INJECTION XU10J4R BVM DEPOL 15-04 UP TO O 7146 - INJECTION XU10J4R BVA DEPOL 15-04 UP TO O 7664
| 0135 0N | 01 | MARK RFV - INJECTION XU10J4R BVM EXCEPT DEPOL 15-04 SINCE O 7147 UP TO O 7664
| 0139 T7 | 01 | EXCHANGE ENGINE MARK RFV - INJECTION XU10J4R BVM EXCEPT DEPOL 15-04 SINCE O 7147 UP TO O 7664
| 0135 1Q | 01 | NEW ENGINE MARK RFV - INJECTION XU10J4R BVM EXCEPT DEPOL 15-04 SINCE O 7665
| 0135 3Q | 01 | MARK RFV - INJECTION XU10J4R BVA EXCEPT DEPOL 15-04 SINCE O 7665
| 0135 5H | 01 | MARK R6E - INJECTION XU10J4R BVM DEPOL 15-04 SINCE O 7147 UP TO O 7664
| 0135 2Q | 01 | MARK R6E - INJECTION XU10J4R BVM DEPOL 15-04 SINCE O 7665
| 0135 4Q | 01 | MARK R6E - INJECTION XU10J4R BVA DEPOL 15-04 SINCE O 7665
| 0143 F6 | 01 | SCHARGE ENGINE