GB |
Z7F 6 60C01B | MAIN WIRING UNDER BONNET

LEFT HAND DRIVE EXCEPT TURBO DIESEL DK5ATE EXCEPT INJECTION ES9J4

01 | 6502 YY | 01 | MAIN HARNESS MARK 9620993880 - ENGINE WATER TEMPERATURE SWITCH WITHOUT SPEED CONTROL WITHOUT THEFT PROTECTION ALARM STANDARD IGNITION UP TO S 91013139

6502 2R

01

MARK
9621425180
9623474780
9623474880
- ENGINE WATER TEMPERATURE SWITCH SPEED CONTROL UP TO S 91013139
- ENGINE WATER TEMPERATURE SWITCH WITH THEFT PROTECTION ALARM UP TO S 91013139
- ENGINE WATER TEMPERATURE SWITCH CODED IGNITION UP TO S 91013139
- ENGINE WATER TEMPERATURE SWITCH SINCE S 91013140

| 6502 ZA | 01 |
| RP 6502 2N | 01 | MARK 9621425280 9621425480 - ENGINE WATER TEMPERATURE BOX EXCEPT (J) UP TO S 91013139
| 6502 2N | 01 | MARK 9623474980 9623475080 - ENGINE WATER TEMPERATURE BOX EXCEPT (J) SINCE S 91013140 UP TO O 6929

6507 C1

01

MARK
9625694980
9625695180
9626436380
9626436580
9629099580
9629099780
- ENGINE WATER TEMPERATURE BOX EXCEPT (J) SINCE O 6930 UP TO O 7510

| 6507 LN | 01 | MARK 9630269680 - ENGINE WATER TEMPERATURE BOX EXCEPT (J) SINCE O 7511 UP TO O 7692

6507 RR

01

MARK
9632122080
9632122180
9633310880
9633310980
- ENGINE WATER TEMPERATURE BOX EXCEPT (J) SINCE O 7693

| 6502 2S | 01 | MARK 9621425680 - ENGINE WATER TEMPERATURE BOX (J) UP TO O 6929
| 6507 C3 | 01 | MARK 9625695380 - ENGINE WATER TEMPERATURE BOX (J) SINCE O 6930 UP TO O 7069
| 6507 HJ | 01 | MARK 9626436780 9629099980 - ENGINE WATER TEMPERATURE BOX (J) SINCE O 7070
10 | 6555 C1 | 01 | CONDENSER 220 UF
11 | 6555 PY | 01 | HARNESS BRACKET
13 | 6547 S8 | 01 | BOX BRACKET
14 | 6555 SQ | 01 |
20 | 6555 T1 | 01 | HARNESS CLIP DIAM 13 A 19
21 | 6555 Z3 | 01 | DIAM 28
38 | 6983 60 | 01 | PLUG
39 | 6983 59 | 01 | WIRING SHEATH 22-70-45
40 | 6555 GF | 01 | RIGHT DRAFTEX - EXCEPT WITH ABS BRAKES
| 6555 GE | 01 | RIGHT DRAFTEX - WITH ABS BRAKES
41 | 6555 GC | 01 | LEFT DRAFTEX
71 | 6980 33 | 03 | STRAP LONG=150 LARG=7
72 | 6980 44 | 02 | LONG 163 LARG 5
73 | 6980 47 | 04 | LONG 171 LARG 9
74 | 6997 52 | 06 | 13-44
75 | 6992 A8 | 01 | CLIP 1,5-3--6,5
76 | 6995 05 | 01 |
77 | 6997 53 | 05 |
78 | 6992 G7 | 01 | DIAM 11-20
| RP 6992 H3 | 01 |