GB |
Z7F 8 89W01A | FRONT SAFETY BELTS

WITHOUT TITLE

01 | 8972 N1 LE-9702 | 01 | PYROTEC BELT FXX BLACK - "FT" UP TO O 6537
| 8972 T8 LE-9703 | 01 | FXX BLACK - "FT" SINCE O 6538
| 8972 N2 LE | 01 | FCY IMPALA BEIGE - "FC" UP TO O 6537
| 8972 T9 LE-9901 | 01 | FCY IMPALA BEIGE - "FC" SINCE O 6538 UP TO O 7509 - "FG" UP TO O 7509
| 8972 PR | 01 | LEFT FEX CASSEL EARTH BEIGE - "FD" SINCE O 7510
| 8972 PS | 01 | RIGHT FEX CASSEL EARTH BEIGE - "FD" SINCE O 7510
02 | 8978 G4 | 02 | FIXING COVER FZG LIGHT GREY - "FT"
| 8978 G2 | 02 | FCZ IMPALA BEIGE - "FC" UP TO O 7509 - "FG" UP TO O 7509
| 8978 FL | 02 | FEX CASSEL EARTH BEIGE - "FD" SINCE O 7510
03 | 8978 G7 | 02 | CONTROL BUTTON FZG LIGHT GREY - "FT"
| 8978 G5 | 02 | FCZ IMPALA BEIGE - "FC" UP TO O 7509 - "FG" UP TO O 7509
| 8978 FK | 02 | FEX CASSEL EARTH BEIGE - "FD" SINCE O 7510
04 | 8978 G8 | 02 | BELT GUIDE RAMP
05 | 8978 G9 | 02 | BELT SCREW H 7/16"X20-8,5
| RP 8978 EF | 01 |
06 | 8978 H1 | 02 | 7/16X20-16
07 | 8978 F9 | 02 | WASHER-SCREW 7/16X20X25
08 | 8971 20 | 02 | BELT SCREW H 7/16"X20-10,5
09 | 8978 S0 | 02 | FLEXIBLE WASHER 13,2X25-1
10 | 6555 P5 | 02 | HSG SEAT BELTS UP TO O 6601
| 6555 SJ | 01 | SINCE O 6601
70 | 6922 22 | 04 | SELF-TAP SCREWS 8X125-20
71 | 6936 62 | 04 | NUT WITH BASE 6X100-7,4-10