GB |
Z7F 5 50A01A | FRONT SPRING FRONT TORSION BAR

NORMAL SUSPENSION
UP TO O 7510

01

5002 G0

02

SUSPENSN SPRING
- CARBURETTOR XU102C
- INJECTION XU10J2 BVM LEVEL 1 W/O ABS BRAKES
- INJECTION XU10J2 BVM LEVEL 2 WITHOUT AIR CONDITIONING
- INJECTION XU10J4R LEVEL 1
- INJECTION XU10J4R BVM LEVEL 2
- INJECTION XU10J4R BVA LEVEL 2 WITHOUT AIR CONDITIONING
2 RED OR 1 GREEN

5002 G1

02

- INJECTION XU10J2 BVM LEVEL 1 WITH ABS BRAKES
- INJECTION XU10J2 BVA LEVEL 1 W/O ABS BRAKES
- INJECTION XU10J2 BVM LEVEL 2 AIR CONDITIONING
- INJECTION XU10J2 BVA LEVEL 2 W/O ABS BRAKES WITHOUT AIR CONDITIONING
- INJECTION XU10J2 BVM LEVEL 3 W/O ABS BRAKES
- INJECTION XU10J4R BVA LEVEL 2 AIR CONDITIONING
- TURBO INJECTION XU10J2TE BVM LEVEL 2 WITHOUT AIR CONDITIONING
- TURBO INJECTION XU10J2TE BVM LEVEL 2 W/O ABS BRAKES AIR CONDITIONING
- TURBO INJECTION XU10J2TE BVA LEVEL 2 W/O ABS BRAKES WITHOUT AIR CONDITIONING
- TURBO DIESEL XUD11BTE BVM LEVEL 1
- TURBO DIESEL XUD11ATE BVM LEVEL 1 WITHOUT AIR CONDITIONING
3 RED OR 2 GREEN

5002 G2

02

- INJECTION XU10J2 BVA LEVEL 1 WITH ABS BRAKES
- INJECTION XU10J2 BVA LEVEL 2 WITH ABS BRAKES
- INJECTION XU10J2 BVA LEVEL 2 W/O ABS BRAKES AIR CONDITIONING
- INJECTION XU10J2 BVM LEVEL 3 WITH ABS BRAKES
- INJECTION XU10J2 BVA LEVEL 3 W/O ABS BRAKES
- TURBO INJECTION XU10J2TE BVM LEVEL 2 WITH ABS BRAKES AIR CONDITIONING
- TURBO INJECTION XU10J2TE BVA LEVEL 2 WITH ABS BRAKES WITHOUT AIR CONDITIONING
- TURBO INJECTION XU10J2TE BVA LEVEL 2 W/O ABS BRAKES AIR CONDITIONING
- TURBO DIESEL XUD11ATE BVM LEVEL 1 AIR CONDITIONING
- TURBO DIESEL XUD11ATE BVA LEVEL 1 W/O ABS BRAKES WITHOUT AIR CONDITIONING
- TURBO DIESEL XUD11ATE BVM LEVEL 2 W/O ABS BRAKES AIR CONDITIONING
- TURBO DIESEL XUD11BTE BVM LEVEL 2 W/O ABS BRAKES WITHOUT AIR CONDITIONING
- TURBO DIESEL XUD11ATE BVA LEVEL 2 W/O ABS BRAKES WITHOUT AIR CONDITIONING
- TURBO DIESEL XUD11ATE BVM LEVEL 2 WITHOUT AIR CONDITIONING
4 RED OR 3 GREEN

5002 G3

02

- INJECTION XU10J2 BVA LEVEL 3 WITH ABS BRAKES
- TURBO INJECTION XU10J2TE BVA LEVEL 2 WITH ABS BRAKES AIR CONDITIONING
- TURBO DIESEL XUD11BTE BVA LEVEL 1
- TURBO DIESEL XUD11BTE BVM LEVEL 2 WITH ABS BRAKES AIR CONDITIONING
- TURBO DIESEL XUD11BTE BVA LEVEL 2
- TURBO DIESEL XUD11ATE BVA LEVEL 1 WITH ABS BRAKES WITHOUT AIR CONDITIONING
- TURBO DIESEL XUD11ATE BVA LEVEL 1 AIR CONDITIONING
- TURBO DIESEL XUD11ATE BVM LEVEL 2 WITH ABS BRAKES AIR CONDITIONING
- TURBO DIESEL XUD11ATE BVA LEVEL 2 WITH ABS BRAKES WITHOUT AIR CONDITIONING
5 RED OR 4 GREEN
- TURBO DIESEL XUD11ATE BVA LEVEL 2 AIR CONDITIONING

| 5002 G4 | 02 | - INJECTION ZPJ BVM - INJECTION ZPJ BVA WITHOUT AIR CONDITIONING 6 RED OR 5 GREEN
| 5002 G5 | 02 | - TURBO DIESEL XUD11BTE BVM LEVEL 3 - INJECTION ZPJ BVA AIR CONDITIONING - TURBO DIESEL XUD11ATE BVM LEVEL 3 1 GREEN + 1 RED OR 6 GREEN - TURBO DIESEL DK5ATE LEVEL 2
| 5002 G6 | 02 | - TURBO DIESEL XUD11BTE BVA LEVEL 3 - TURBO DIESEL XUD11ATE BVA LEVEL 3 1 GREEN + 2 RED OR 1 RED
| 5002 G9 | 02 | - TURBO DIESEL DK5ATE LEVEL 3 1 GREEN + 3 RED OR 2 GREEN + 1 RED
02 | 5254 22 | 02 | ROD PROTECTOR CONTIN GU.WERKE
03 | 5033 40 | 02 | REBOUND STOP DIAM 56 H=109 ELASTOGRAN
04 | 5035 32 | 02 | NEEDLE ROLLER
05 | 5038 20 | 02 | SHOCK-AB BRACKT
06 | 5033 46 | 02 | REST CUP
07 | 5033 47 | 02 | CONTROL CUP
08 | 5037 28 | 02 | SHEATH
09 | 5209 10 | 02 | CLEANER PLUG DIAM 19,5X25,5 E =22
10 | 5031 35 | 02 | MOUNTING ASSY
11 | 5033 50 | 02 | SEAL ELASTIQ SACRED
70 | 5036 05 | 06 | CAPSCREW HM 8X125_20
71 | 6947 78 | 06 | PLAIN WASHER 8X16-1,5
72 | 6949 11 | 04 | 14X38-3
73 | 6939 91 | 02 | SELF LOCKG NUT 14X150-13-21