GB |
Z7F 5 51A55A | SUSP CROSSMEMBR TORSION BAR RECESS DOOR

SINCE O 7511

01 | 5102 87 | 02 | SUSPENSN SPRING - TURBO DIESEL DK5ATE LEVEL A NORMAL SUSPENSION 1 RED + 1 GREEN OR 2 GREEN
| 5102 89 | 02 | - TURBO INJECTION XU10J2TE LEVEL A NORMAL SUSPENSION - INJECTION ES9J4 LEVEL B NORMAL SUSPENSION 1 RED + 1 YELLOW OR 2 RED

5102 90

02

- INJECTION ES9J4 LEVEL A NORMAL SUSPENSION
- INJECTION XU10J4R LEVEL A NORMAL SUSPENSION
- INJECTION XU10J4R BVM LOW / HIGH NORMAL SUSPENSION
- TURBO DIESEL XUD11BTE LEVEL A NORMAL SUSPENSION
- TURBO DIESEL XUD11BTE BVM LOW / HIGH NORMAL SUSPENSION
- TURBO DIESEL DK5ATE LEVEL B NORMAL SUSPENSION
1 BLUE + 1 RED OR 2 BLUE

| 5102 96 | 02 | - INJECTION XU10J4R LEVEL A FR/RR HEAVY DUTY SUSPENSION 2 GREEN + 1 RED OR 2 GREEN + 1 YELLOW
| 5102 97 | 02 | - INJECTION ES9J4 LEVEL B FR/RR HEAVY DUTY SUSPENSION 1 YELLOW + 1 BLUE OR 1 YELLOW
02 | 5164 32 | 02 | WASHER UP TO O 7629
03 | 5165 26 | 02 | SPRING SUPPORT UP TO O 7629
| 5164 34 | 02 | SOCAT SINCE O 7630