GB |
Z7F 1 11A20A | ENGINE OIL SUMP FILTER PROBE

INJECTION ZPJ INJECTION ZPJ4

01 | 1109 87 | 01 | OIL FILTER
02 | 1103 53 | 01 | OIL FILT INSERT
03 | 1103 91 | 01 | DISTRIB CHAMBER
04 | 1104 19 | 01 | SEAL 62,3X71,8-4,75 VALEO THERMIQUE -
05 | 1103 74 | 01 | OIL FILT INSERT
06 | 1103 94 | 01 | STOP PLATE
07 | 1171 63 | 01 | OIL GAUGE GUIDE - INJECTION ZPJ UP TO M 51769 - INJECTION ZPJ4
| 1171 94 | 01 | - INJECTION ZPJ SINCE M 51770
08 | 1174 06 | 01 | ENGINE OIL GAUG - INJECTION ZPJ UP TO M 51769 - INJECTION ZPJ4
| 1174 32 | 01 | - INJECTION ZPJ SINCE M 51770
09 | 1462 01 | 01 | ELASTIC BRACKET - INJECTION ZPJ UP TO M 51769 - INJECTION ZPJ4
10 | 1170 19 | 01 | RING-SEAL - INJECTION ZPJ UP TO M 51769 - INJECTION ZPJ4
| 1170 26 | 01 | - INJECTION ZPJ SINCE M 51770
11 | 1131 68 | 01 | OIL LEVEL PROBE
| RP 1131 A2 | 01 | - INJECTION ZPJ UP TO M 52079 - INJECTION ZPJ4 UP TO M 9150
| 1131 A2 | 01 | - INJECTION ZPJ SINCE M 52080 - INJECTION ZPJ4 SINCE M 9151
12 | 1131 60 | 01 | SCREW COLUMN
13 | 1131 65 | 01 | CAPSCREW
14 | 1131 62 | 01 | SPACER
15 | 1131 82 | 01 | OIL PRES SWITCH 16X150 JAEGER SOBINT
16 | 0301 C7 | 01 | ENGINE OIL SUMP
17 | 1338 09 | 01 | TEMPERATURE 110 DEG JAEGER BE BLUE
18 | 0309 02 | 01 | NUT SOCKET
19 | 0310 02 | 01 | SQUARE NUT 16X150-8
20 | 0164 30 | 01 | PLUG SEAL 16X22-2 A005 WITHOUT ASBESTOS
21 | 0163 21 | 01 | CASING PLUG 16X150-12
22 | 1049 04 | 01 | SUCTION PIPE
23 | 1047 05 | 01 | PANEL
25 | 0609 07 | 03 | PISTON OIL JET AV
| 0609 08 | 03 | AR
70 | 6915 69 | 20 | CAPSCREW 6X100-16
| RP 6917 A5 | 02 |
71 | 6922 80 | 08 | SELF-TAP SCREWS 6X100-25
72 | 6922 29 | 06 | SCREW WITH BASE 6X100-35
73 | 6922 73 | 02 | SELF-TAP SCREWS 6X100-12 SINCE M 51770