GB |
Z7F 1 10A15A | ENGINE OIL PUMP CHAIN BELT SUCTION

INJECTION XU10J4R

01 | 1001 77 | 01 | ENGINE OIL PUMP
02 | 1018 43 | 01 | OIL SUCTION
03 | 1011 11 | 01 | PUMP FIX SCREW 7X100-70
04 | 1012 07 | 01 | OIL PUMP SPACER EP 1,1
05 | 1133 13 | 01 | DISCHARG PISTON DIAM 16X25 FORMER
06 | 1157 11 | 01 | PISTON SPRING 6 BARS
07 | 1033 10 | 01 | OIL PUMP CHAIN 52 LINKS
08 | 1047 08 | 01 | PANEL
09 | 1047 11 | 01 | - BVM WITHOUT AIR CONDITIONING UP TO O 7146 - BVA WITHOUT AIR CONDITIONING
| 1047 10 | 01 | - BVM WITHOUT AIR CONDITIONING SINCE O 7147 - AIR CONDITIONING
10 | 1011 12 | 01 | SELF-TAP SCREWS 7X100-85
11 | 1011 14 | 01 | SCREW 7X100-75
12 | 1157 19 | 01 | GUIDE PIN
13 | 0163 78 | 02 | PLUG 16X150
70 | 6922 80 | 06 | SELF-TAP SCREWS 6X100-25
71 | 6922 54 | 02 | 6 X 100 - 20